Falconfig is a CPX module that allows you to control various options available in the Falcon030 including: Toggle CPU between 8 Mhz and 16 Mhz, Toggle Blitter between 8 Mhz and 16 Mhz, Turn the CPU cache on and off, Set internal IDE hard drive, Toggle between 78 Hz / 60 Hz (this feature is only available when "Super 78" is installed). All docs are in German.

Information

|  |  |
| --- | --- |
| **Version/Release date:** | 1.07 06/06/1993 |
| **Systems:** | Atari Falcon |
| **Status:** | Freeware |
| **Programmer** | [Christoph Wissing](https://www.atariuptodate.de/en/authors/christoph-wissing-3005/) |
| **Compatibility:** | ◇ ST ◇ STE ◇ TT ◆ [Falcon](https://www.atariuptodate.de/en/falcon/) ◈ CT60 ◈ Hades ◈ Milan ◈ FireBee |
| **Resolutions:** | all |
| **Type:** | CPX module |

Availability

|  |  |
| --- | --- |
| **Availability:** | [ST-Computer PD 996](https://www.st-computer.org/publicdomain/stcpd996.zip)[[?]](http://tho-otto.de/fatfs/fatfs.php?image=https%3A%2F%2Fwww.st-computer.org%2Fpublicdomain%2Fstcpd996.zip) (Falconfig) |
| **CD-ROMs:** | Crawly Crypt 2 (Falconfig 1.07) |