Overview | Package | Class | Use | Tree | Deprecated | Index | Help
PREV NEXT | FRAMES NO FRAMES

## Uses of Package
org.opengis.referencing.crs

Packages that use org.opengis.referencing.crs
org.opengis.coverage | Coverages (generate a value for any point).
org.opengis.coverage.grid | Quadrilateral grid coverages.
org.opengis.coverage.grid.quadrilateral |
org.opengis.feature | Representation a features on a map.
org.opengis.feature.simple |
org.opengis.feature.type | Captures the generic feature model from ISO 19109 with allowances for usability.
org.opengis.geometry | Root package for geometries.
org.opengis.geometry.coordinate | Set of geometric objects.
org.opengis.geometry.primitive | Set of geometric objects that are not decomposed further into other primitives.
org.opengis.go |
org.opengis.go.display.canvas |
org.opengis.go.display.primitive |
org.opengis.layer | Basic unit of geographic information that may be requested as a map from a server.
org.opengis.metadata.extent | Extent information.
org.opengis.referencing.crs | Coordinate reference systems (coordinate systems with a datum).
org.opengis.referencing.operation | Coordinate operations (relationship between any two coordinate reference systems).

Classes in org.opengis.referencing.crs used by org.opengis.coverage
CoordinateReferenceSystem Abstract coordinate reference system, usually defined by a coordinate system and a datum.

Classes in org.opengis.referencing.crs used by org.opengis.coverage.grid
CoordinateReferenceSystem Abstract coordinate reference system, usually defined by a coordinate system and a datum.

Classes in org.opengis.referencing.crs used by org.opengis.coverage.grid.quadrilateral
CoordinateReferenceSystem Abstract coordinate reference system, usually defined by a coordinate system and a datum.

Classes in org.opengis.referencing.crs used by org.opengis.feature
CoordinateReferenceSystem Abstract coordinate reference system, usually defined by a coordinate system and a datum.
CRSFactory Builds up complex coordinate reference systems from simpler objects or values.

Classes in org.opengis.referencing.crs used by org.opengis.feature.simple
CoordinateReferenceSystem Abstract coordinate reference system, usually defined by a coordinate system and a datum.

Classes in org.opengis.referencing.crs used by org.opengis.feature.type
CoordinateReferenceSystem Abstract coordinate reference system, usually defined by a coordinate system and a datum.
CRSFactory Builds up complex coordinate reference systems from simpler objects or values.

Classes in org.opengis.referencing.crs used by org.opengis.geometry
CoordinateReferenceSystem Abstract coordinate reference system, usually defined by a coordinate system and a datum.

Classes in org.opengis.referencing.crs used by org.opengis.geometry.coordinate
CoordinateReferenceSystem Abstract coordinate reference system, usually defined by a coordinate system and a datum.

Classes in org.opengis.referencing.crs used by org.opengis.geometry.primitive
CoordinateReferenceSystem Abstract coordinate reference system, usually defined by a coordinate system and a datum.

Classes in org.opengis.referencing.crs used by org.opengis.go
CoordinateReferenceSystem Abstract coordinate reference system, usually defined by a coordinate system and a datum.
CRSAuthorityFactory Creates coordinate reference systems using authority codes.
CRSFactory Builds up complex coordinate reference systems from simpler objects or values.

Classes in org.opengis.referencing.crs used by org.opengis.go.display.canvas
CoordinateReferenceSystem Abstract coordinate reference system, usually defined by a coordinate system and a datum.

Classes in org.opengis.referencing.crs used by org.opengis.go.display.primitive
CoordinateReferenceSystem Abstract coordinate reference system, usually defined by a coordinate system and a datum.

Classes in org.opengis.referencing.crs used by org.opengis.layer
CoordinateReferenceSystem Abstract coordinate reference system, usually defined by a coordinate system and a datum.

Classes in org.opengis.referencing.crs used by org.opengis.metadata.extent
VerticalCRS A 1D coordinate reference system used for recording heights or depths.

Classes in org.opengis.referencing.crs used by org.opengis.referencing.crs
CompoundCRS A coordinate reference system describing the position of points through two or more independent coordinate reference systems.
CoordinateReferenceSystem Abstract coordinate reference system, usually defined by a coordinate system and a datum.
DerivedCRS A coordinate reference system that is defined by its coordinate conversion from another coordinate reference system but is not a projected coordinate reference system.
EngineeringCRS A contextually local coordinate reference system.
GeneralDerivedCRS A coordinate reference system that is defined by its coordinate conversion from another coordinate reference system (not by a datum).
GeocentricCRS A 3D coordinate reference system with the origin at the approximate centre of mass of the earth.
GeodeticCRS A coordinate reference system associated with a geodetic datum.
GeographicCRS A coordinate reference system based on an ellipsoidal approximation of the geoid; this provides an accurate representation of the geometry of geographic features for a large portion of the earth's surface.
ImageCRS An engineering coordinate reference system applied to locations in images.
ProjectedCRS A 2D coordinate reference system used to approximate the shape of the earth on a planar surface.
SingleCRS Abstract coordinate reference system, consisting of a single Coordinate System and a single Datum (as opposed to Compound CRS).
TemporalCRS A 1D coordinate reference system used for the recording of time.
VerticalCRS A 1D coordinate reference system used for recording heights or depths.

Classes in org.opengis.referencing.crs used by org.opengis.referencing.operation
CoordinateReferenceSystem Abstract coordinate reference system, usually defined by a coordinate system and a datum.

Overview | Package | Class | Use | Tree | Deprecated | Index | Help
PREV NEXT | FRAMES NO FRAMES

Copyright © 1994-2008 Open Geospatial Consortium. All Rights Reserved.