Post Processor- visualization of calculation results.
Buttons
- File open with results of calculation.
- Save the image in graphic format JPEG.
- Save all. Saves results of calculation as JPEG slides in the specified directory.
- Show all. Enters the image in area of the screen. Increase of the image.
- Reduction of the image.
- Increase of the image.
- Top view.
- Bottom view.
- Left view.
- Right view.
- Front view.
- Back view.
- SW isometrik view.
- SE isometrik view.
- NE isometrik view.
- NW isometrik view.
At the left there is an option of the image where it is possible:
- On/off Mesh
- On/off Deformed with the scale factor, which necessary to specify.
- On/off Contour fill color of elements.
- On/off Gradient - smooth transition on colors.
- On/off Nodes label - to show numbering units.
- On/off Elements label - to show numbering elements.
Result - the type of result which we want to see here gets out. It can be displasements, strains, stresses. In brackets the direction ((I) - intensity is underlined). Below a scale of conformity of color to numerical value.