IMG2MAC

This program converts GEM *.IMG files to the Scooter Macro-format *.MAC.
For this the pixels in the GEM image are converted to squares in 
Scooter-PCB. Such a display uses a great deal of memory, but in return 
business logos and other symbols can be represented quite well.

Operation is quite simple: First select the desired IMG file with the 
file-selector. Next you will be asked for the scale. A scale factor of 1 
means that a pixel will be 1*1 Mil in size. The larger the scale, the 
larger the macro will be. Following this the file-selector appears again 
where the path and name of the macro (PICT.MAC by default) should be input. 
Finally you are asked to input the name of the destination layer.

The program is capable of being improved in many ways, e.g. by offering 
memory-saving rectangles, mirroring, target layers etc.
Those who feel like it can optimise the program for themselves. The 
source in GFA-Basic 3.6 is included (with English comments).

Have fun!

-Hubert Kahlert-
