# C128/C64C Video

Seems to be available on the C128 and the C64C (white color). Compatible with cables for the 5 pin D-SUB on C64's.

(at the Computer)

8 PIN DIN (DIN45326) FEMALE at the Computer.

Pin | Name | Dir | Description
--- | --- | --- | ---
1 | LUM |  | Luminance (monochrome video)
2 | GND |  | Ground
3 | AOUT |  | Audio out
4 | VOUT |  | Composite Video out
5 | AIN |  | Audio in (into the SID chip)
6 | n/c | - | Not connected
7 | n/c | - | Not connected
8 | C |  | Chroma

Note: Direction is Computer relative Monitor.

Contributor: | Joakim Ögren

Source: | CBM Memorial Page Pinouts

Copyright © The Hardware Book Team 1996-2004.
May be copied and redistributed, partially or in whole, as appropriate.
Document last modified: 2002-01-10