# Nokia 5110/6110

(at the cellular phone)

NOKIA SPECIAL at the cellular phone.

Pin | Description
--- | ---
1 | VIN CHARGER INPUT VOLTAGE 8.4V 0.8A
2 | CHRG CTRL CHARGER CONTROL PWM 32Khz
3 | XMIC MIC INPUT 60mV - 1V
4 | SGND SIGNAL GROUND
5 | XEAR EAR OUTPUT 80mV - 1V
6 | MBUS 9600 B/S
7 | FBUS_RX 9.6 - 230.4 KB/S
8 | FBUS_TX 9.6 - 230.4 KB/S
9 | L_GND CHARGER / LOGIC GND

Contributor: | Joakim Ögren

Source: | Nokia 5110/6110 pinout at Technick.net

Copyright © The Hardware Book Team 1996-2004.
May be copied and redistributed, partially or in whole, as appropriate.
Document last modified: 2002-01-10