# Amiga to C1084 Monitor

(to the Amiga)
(at the Monitor)

23 PIN D-SUB FEMALE to the Amiga.
6 PIN DIN MALE at the Monitor.

| Amiga | C1084 |
--- | --- | --- | ---
R | 3 | 4 | R
G | 4 | 1 | G
B | 5 | 5 | B
SYNC | 10 | 2 | HSYNC
GND | 16 | 3 | GND

Contributor: | Joakim Ögren

Source: | Usenet posting in sfnet.harrastus.elektroniikka, Philips 1084 monarin kytkenta by Kari Hautanen

Copyright © The Hardware Book Team 1996-2004.
May be copied and redistributed, partially or in whole, as appropriate.
Document last modified: 2002-01-10