# Serial Printer (9-25)

Use this cable between two a computer (DTE) and a printer (DTE) devices.

(To Computer).
(To Printer).

9 PIN D-SUB FEMALE to Computer.
25 PIN D-SUB FEMALE to Printer.

| D-Sub 1 | D-Sub 2 |
--- | --- | --- | ---
Receive Data | 3 | 3 | Transmit Data
Transmit Data | 2 | 2 | Receive Data
Clear To Send + Data Set Ready | 8 + 6 | 20 | Data Terminal Ready
Carrier Detect + Data Terminal Ready | 1 + 4 |  |
Ground | 5 | 7 | Ground

Contributor: | Joakim Ögren

Source: | ?

Copyright © The Hardware Book Team 1996-2004.
May be copied and redistributed, partially or in whole, as appropriate.
Document last modified: 2002-01-10