# VGA (9)

VGA=Video Graphics Adapter or Video Graphics Array.
Videotype: Analogue.

(at the videocard)
(at the monitor cable)

9 PIN D-SUB FEMALE at the videocard.
9 PIN D-SUB MALE at the monitor cable.

Pin | Name | Dir | Description
--- | --- | --- | ---
1 | RED |  | Red Video
2 | GREEN |  | Green Video
3 | BLUE |  | Blue Video
4 | HSYNC |  | Horizontal Sync
5 | VSYNC |  | Vertical Sync
6 | RGND |  | Red Ground
7 | GGND |  | Green Ground
8 | BGND |  | Blue Ground
9 | SGND |  | Sync Ground

Note: Direction is Computer relative Monitor.

Contributor: | Joakim Ögren

Source: | ?

Copyright © The Hardware Book Team 1996-2004.
May be copied and redistributed, partially or in whole, as appropriate.
Document last modified: 2002-01-13