# Atari Floppy Port

(at the Computer)
(at the Diskdrive)

14 PIN DIN FEMALE at the Computer.
14 PIN DIN MALE at the Diskdrive.

Pin | Name | Description
--- | --- | ---
1 | RD | Read Data
2 | SIDE0 | Side 0 Select
3 | GND | Ground
4 | INDEX | Index
5 | SEL0 | Drive 0 Select
6 | SEL1 | Drive 1 Select
7 | GND | Ground
8 | MOTOR | Motor On
9 | DIR | Direction In
10 | STEP | Step
11 | WD | Write Data
12 | WG | Write Gate
13 | TRK00 | Track 00
14 | WP | Write Protect

Contributor: | Joakim Ögren, Lawrence Wright, Steve & Sally Blair

Source: | ?

Copyright © The Hardware Book Team 1996-2004.
May be copied and redistributed, partially or in whole, as appropriate.
Document last modified: 2002-01-10