# Commodore 1084 & 1084S (Digital)

(at the Monitor)

8 PIN DIN 'C' FEMALE at the Monitor.

Pin | Name | Description
--- | --- | ---
1 | n/c | Not connected
2 | R | Red
3 | G | Green
4 | B | Blue
5 | I | Intensity
6 | GND | Ground
7 | HSYNC | Horizontal Sync
8 | VSYNC | Vertical Sync

Contributor: | Joakim Ögren

Source: | National Amiga's C1084 page

Copyright © The Hardware Book Team 1996-2004.
May be copied and redistributed, partially or in whole, as appropriate.
Document last modified: 2002-01-10