# WTX 12V CPU (P4/P5)

12 PIN MOLEX 39-29-9062 CONNECTOR at the Motherboard
12 PIN MOLEX 39-30-1060 CONNECTOR at the cable

Pin | Name |  | Color | Description | AWG
--- | --- | --- | --- | --- | ---
1 | 12Vcpu# |  | White | +12 VDC (CPU) | 18
2 | 12Vcpu# |  | White | +12 VDC (CPU) | 18
3 | 12Vcpu# |  | White | +12 VDC (CPU) | 18
4 | com |  | Black | Ground | 18
5 | com |  | Black | Ground | 18
6 | com |  | Black | Ground | 18

Contributor: | Joakim Ögren

Source: | WTX Power Supply Design Guidelines at WTX Website

Copyright © The Hardware Book Team 1996-2004.
May be copied and redistributed, partially or in whole, as appropriate.
Document last modified: 2002-01-10