# Motherboard Power

(at the Computer)
(at the Powersupply cables)

2x MOLEX 15-48-0106 CONNECTOR at the Computer.
2x MOLEX 90331-0001 CONNECTOR at the Powersupply cables.

## P8

Pin | Name |  | Color | Description
--- | --- | --- | --- | ---
1 | PG |  | Orange | Power Good, +5 VDC when all voltages has stabilized.
2 | +5V |  | Red | +5 VDC (or n/c)
3 | +12V |  | Yellow | +12 VDC
4 | -12V |  | Blue | -12 VDC
5 | GND |  | Black | Ground
6 | GND |  | Black | Ground

## P9

Pin | Name |  | Color | Description
--- | --- | --- | --- | ---
1 | GND |  | Black | Ground
2 | GND |  | Black | Ground
3 | -5V |  | White or Yellow | -5 VDC
4 | +5V |  | Red | +5 VDC
5 | +5V |  | Red | +5 VDC
6 | +5V |  | Red | +5 VDC

Note: Pins part number is 08-50-0276, Product specification is PS-90331.

Contributor: | Joakim Ögren, Bill Shepherd

Source: | ?

Copyright © The Hardware Book Team 1996-2004.
May be copied and redistributed, partially or in whole, as appropriate.
Document last modified: 2002-01-10