# AAUI to AUI

Is the directions right???

(to the Macintosh)
(to the Transciever)

14 PIN UNKNOWN CONNECTOR to the Macintosh (AAUI)
15 PIN D-SUB FEMALE to the Transciever (AUI)

Description | AAUI | AUI
--- | --- | ---
control in circuit A | 5 | 2
data out circuit A | 9 | 3
data in circuit shield | shell | 4
data in circuit A | 2 | 5
voltage common | 4 | 6
control out circuit shield | shell | 8
control in circuit B | 6 | 9
data out circuit B | 10 | 10
data out circuit shield | shell | 11
data in circuit B | 3 | 12
voltage plus | 1 | 13
voltage shield | shell | 14

Contributor: | Joakim Ögren

Source: | Apple Tech Info Library 9980: AAUI, Pinout Equivalents to AUI at Apple TIL homepage

Copyright © The Hardware Book Team 1996-2004.
May be copied and redistributed, partially or in whole, as appropriate.
Document last modified: 2002-01-13