# Apple S-Video Input

(at the computer)

7 PIN SPECIAL MINI-DIN FEMALE at the computer.

Available on Apple Power Macintosh 6100AV/7100AV/8100AV

Pin | Description
--- | ---
1 | Analog GND
2 | Analog GND
3 | Video Y (Luminance)
4 | Video C (Chroma)
5 | I2C Clock
6 | +12 VDC (max 250mA)
7 | I2C Data

Contributor: | Joakim Ögren

Source: | ?

Copyright © The Hardware Book Team 1996-2004.
May be copied and redistributed, partially or in whole, as appropriate.
Document last modified: 2002-01-10