# Amiga 1000 RF Monitor

(at the computer)

8 PIN DIN "C" FEMALE at the computer.

Pin | Name | Dir | Description
--- | --- | --- | ---
1 | n/c | - | Not connected
2 | GND |  | Ground
3 | AUDL |  | Audio Left
4 | CVIDEO |  | Composite Video
5 | GND |  | Ground
6 | n/c | - | Not connected
7 | +12V |  | +12 VDC
8 | AUDR |  | Audio Right

Note: Direction is Computer relative Monitor.

Contributor: | Joakim Ögren

Source: | ?

Copyright © The Hardware Book Team 1996-2004.
May be copied and redistributed, partially or in whole, as appropriate.
Document last modified: 2002-01-10