# SFX Optional Power

(at the motherboard)
(at the cable)

6 PIN MOLEX 39-30-1060 at the motherboard
6 PIN MOLEX 39-01-2060 at the cable

Pin | Name |  | Color | Description
--- | --- | --- | --- | ---
1 | Reserved |  | n/a |
2 | Fan On/Off |  | White/Blue | Fan Control
3 | Reserved |  | n/a |
4 | Reserved |  | n/a |
5 | Reserved |  | n/a |
6 | Reserved |  | n/a |

Contributor: | Joakim Ögren

Source: | ATX Spec v2.03 at Platform Development Support

Copyright © The Hardware Book Team 1996-2004.
May be copied and redistributed, partially or in whole, as appropriate.
Document last modified: 2002-01-13