# Commodore 1084 & 1084S (Analog) Connector

(at the Monitor)

6 PIN DIN FEMALE at the Monitor.

Pin | Name | Description
--- | --- | ---
1 | G | Green
2 | HSYNC | Horizontal Sync
3 | GND | Ground
4 | R | Red
5 | B | Blue
6 | VSYNC | Vertical Sync

Contributor: | Joakim Ögren

Source: | National Amiga's C1084 page

Copyright © The Hardware Book Team 1996-2004.
May be copied and redistributed, partially or in whole, as appropriate.
Document last modified: 2002-01-10