Atari 810

## Description

First diskette drive made by Atari.

## Picture

here (25 KB JPG)

## Formats

SSSD

## Speeds

19.2 kbps

## RPM

288

## Hardware

cpu 6507, riot 6532, wd1771 fdc, ram 6810, two SIO ports. Memory map (0 KB TXT).

## Schematics

Rear board (36 KB GIF), side board (67 KB GIF), drawn by Jerzy Sobola.

# Upgrades

## 810 Archiver

Copies many copy-protected programs

## Happy 810

Manufacturer: Happy Computer
Happy Backup, Warp Speed 52kbps, 18 sector buffer

## Fast Chip

Manufacturer: Binary
10-40% faster than stock drive

## 810 Turbo

Manufacturer: Neanderthal Computer Things
double density Back (c) 1998-2004 Jindroush Last modified: Sat Jan 11 22:53:56 2003