Atari Falcon030 capacitor set

Complete set of capacitors for complete Atari recap, Falcon030 mainboard specific bundle.

Top of Form

Description

This re-cap set consists of following electrolytic capacitors:

1\* 4700uF/10V, THT, Ø16x37mm, axial (C147 )  
1\* 470uF/16V, THT, Ø8x20mm, axial (C24)  
2\* 220uF/16V, THT, Ø8x16mm, axial (C57,C121)  
1\* 220uF/16V, THT, Ø6,3x11mm, radial (C117)  
4\* 100uF/25V, THT, Ø6,3x16mm, axial (C29,C36,C50,C110)  
5\* 47uF/25V, THT, Ø6,3x12mm, axial (C54,C56,C67,C83,C84,C138)  
1\* 22uF/50V, THT, Ø6,3x12mm, axial (C1)  
3\* 10uF/63V, THT, Ø5x12mm, axial (C88,C91,C114,C141)  
2\* 4,7uF/100V, THT, Ø5x12mm, axial (C2,C6)  
4\* 3,3uF/100V, THT, Ø5x12mm, axial (C92,C127)  
1\* 2,2uF/100V, THT, Ø5x12mm, axial (C78)  
3\* 1uF/100V, THT, Ø5x12mm, axial (C48,C101,C181)